ARCHITECTURAL SPECIFICATIONS
OUTLINE Ai81

The loudspeaker shall be a 9-transducer, one-channel, 2-way, passive, low-distortion column array device.
The transducers shall consist in eight 1.3-inch Neodymium magnet woofers in a column array arrangement and 0.7-inch treated silk dome tweeter with ferrofluid in air gap.
The lightweight cabinet shall be constructed in HCDF (Hydrophobic Compact Density Fiber). It shall be coated with textured polyurethane paint. The grill shall be of galvanized steel with an epoxy powder coating. The model shall have custom repainting RAL options.
The unit shall feature two through holes and three threaded points to allow flexible installations and mounting options.
The loudspeaker shall have a companion subwoofer that ensure the extension of low end reproduction with the same tonal balance.
The connector of the loudspeaker shall be one 2-pin Euroblock captive screw terminal.
The loudspeaker shall employ an internal cross-over network manufactured with top-grade miniature components. The system shall include a bulb for tweeter protection.
The unit shall have a DSP presets available on the suggested amplifier with all the processing and protections needed.
The frequency response shall be 300 Hz to 20 kHz (-10dB).
Maximum peak SPL output for one box shall be 112 dB calculated using +12dB crest factor signal @ 1m, Half space (AES2-2012).
The nominal acoustic dispersion of a single cabinet shall be of 160° horizontal and 40° vertical.
The nominal impedance of a single enclosure shall be 16 Ω. The power handling of the box shall be 20 W AES continuous and 320 W AES peak according to AES2-2012 standard.
The enclosure shall have a minimal visual impact and shall not exceed 570 mm (22 4/8”) in height, 46 mm (1 6/8”) in width, 25 mm (1”) in depth and the weight shall be 0.85 Kg (1.85 lb).