ARCHITECTURAL SPECIFICATIONS
OUTLINE VEGAS 15

The loudspeaker shall be a 2-transducer, one-channel, 2-way, passive, low-distortion point source device.
The transducers shall consist of one by fifteen-inch bass reflex loaded woofer and one one-and-seventy-five-inch compression driver mounted on a rotatable moulded horn. 
The lightweight cabinet shall be constructed in 15mm phenolic glued baltic birch plywood.
The cabinet shall be black polyurea coated, and the grille shall have an epoxy powder coating. The cabinet shall have custom repainting RAL options.
The cabinet shall have smoothly finished handles carved in the top and bottom panels of the cabinet to facilitate the general management of the system (transportation, moving as well as installation).
The cabinet shall have four M6 and twelve M8 threaded rigging points to allow flexible installation. The bottom of the cabinet shall have a 35 mm pole mount insert.
The connectors of the loudspeaker shall be one NL4 speakON with one additional pass-through NL4 connector for parallel loudspeaker connections.
The speaker shall employ an internal crossover network manufactured with top-grade components, including coils with very low resistance and metalized polypropylene capacitors.
The frequency response shall be 53 Hz to 20 kHz (-10dB).
Maximum peak SPL output for one box shall be 132 dB calculated using +10dB crest factor signal @ 1m, free field.
The nominal acoustic dispersion of a single cabinet shall be 80° horizontal and 70° vertical with rotatable horn.
The power handling of the box shall be 400 W AES continuous and 1600 W AES peak.
The nominal impedance of the single enclosure shall be 8 Ω.
The enclosure shall be 750 mm (29 17/32”) high, 450 mm (17 23/32”) wide, 390 mm (15 11/32”) deep and the weight shall be 25.8 Kg (56.9 lb).